Balance Calculator Creator Guide

1. Creating the DOE batch
   1. Open your sim file and assemble/setup. Make sure your condition set is selected.
   2. Copy the setup compare.
   3. Hit the “Paste S.C.” button in the app

A screenshot of a computer

AI-generated content may be incorrect.

* 1. The green light will pop up if the paste was successful.
  2. Hit the “Save Batch” button and save it in an accessible place.

1. Running the DOE
   1. Go to the simulation tab and then Metric Options
   2. Load in the segments and the filter set. Segments are created for almost all tracks, will have “7BC” attached. The current calculator template (v1.2) has 6 segment slots. The values can be changed in different corner names are needed, the formulas are based off a xlookup.

A screenshot of a computer program

AI-generated content may be incorrect.

* 1. Go to he DOEs page.
  2. Click the Static tab and choose the following selections:
  3. A screenshot of a computer

     AI-generated content may be incorrect.
  4. Get back to the DOE Batches page. Hit the send button
  5. A group of colorful text

     AI-generated content may be incorrect.
  6. Load in the previously saved batch. And Hit Send

A screenshot of a computer

AI-generated content may be incorrect.

1. Exporting the DOE data.
   1. Recommend to re-load the filter set. Sim has had some issues before where that resets when you do too many things.
   2. Select your DOE on the batch page, and export **both** the summary and the filtered metrics.
2. Running the app
   1. Select the filepath for the filtered metrics and summary in the top left hand corner.

A screenshot of a calculator

AI-generated content may be incorrect.

* 1. Leave “Is SF-1 Split?” checked if the segment has been split into a and b. This has to be done to include the whole front straight in the segments.
  2. Leave the “Save Calculator?” box checked if you want to create a balance calculator. It will be saved in the same directory the metrics were saved to. You can enter a name for it, or if left blank, it will save it as the name of your batch + “\_BC”.
     1. If unchecked, it will fill in the data for the variation plots and nothing else, is considerably faster if you just want to see the plots.
  3. Hit run script.
  4. The script will ask for a template file to save to, select the attached template BC\_Template file. (Current version 1.2).
  5. Once complete, the data for the plots will also be filled out.
  6. A screenshot of a graph

     AI-generated content may be incorrect.
  7. Select the dropdowns to choose what you would like to see plotted. It will either be matched with a 1st degree or 3rd degree curve fit. What is shown is what the calculator will use.
  8. You can hit the “Copy Plot Data” button below the plots to copy the data to clipboard if you would like to export it somewhere else.

1. Using the Balance Calculator.
   1. Note: all values calculated are deltas from baseline.

A screenshot of a computer

AI-generated content may be incorrect.

* 1. Enter your changes into the purple boxes, the gray boxes are your baseline setup values.
     1. Almost every value should be entered as a delta, i.e. if you want to see what change 1 round in the RR would be, just put 1 in the purple box instead of the total.
     2. **The only values that should not be entered as deltas are:**
        1. Blade Positions
        2. RR Rollout Delta
  2. Hit the reset button to clear data, note this is run thru a macro so ctrl+z will not do anything after you hit it.